Note: This API call is for DOS and Win16 personality only. Use Family API for portability.

AH=03H

Version

2 and higher

Brief

Global Enable A20

Family API

none

Input

AH = 03h

Return

AX = 0001h if the A20 line is enabled, 0000h otherwise

BL = Error code

Notes

See also